
SE135-9W履带式液压挖掘机Hydraulic Crawler Excavator
技术规格参数Technical Specifications
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          发动机

Engine
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         行走系统

Travel System

	型号Model
	潍柴Weichai WP4.1
	行走马达Travel motors
	艾迪Eddie FTM22A

	形式Type
	高压共轨,水冷,涡轮增压

High-pressure common rail, water-cooled, turbocharged
	支重轮数量Track roller quantities
	2×7

	
	
	拖链轮数量Carrier roller quantities
	2×1

	缸数No. of cylinder
	4
	履带板数量Travel shoes
	2×44

	缸径×行程Bore and stroke
	105mm×118mm
	行走速度Travel speed
	3.25/5.20km/h

	排量Displacement
	4.1L
	牵引力Drawbar pulling force
	118kN

	额定功率Power output
	92kW/2200rpm
	爬坡能力Grade ability
	70% (35°)

	
	
	离地间隙Ground clearance
	425mm
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   液压系统 Hydraulic System
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      回转系统 Swing System

	液压泵Main Pump
	Hengli
	回转马达Swing motor
	Hengli

	主泵型号Model
	 V90N75DT
	回转马达型号Swing motor type
	 HM5X80CHB

	额定工作流量  

Max.discharge flow
	2×130L/min
	回转速度Swing speed
	0-10r/min

	主阀Main Valve
	Hengli  HVME180B
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           挖掘力

Digging Force (ISO6015)  (Kn)
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      润滑油及容量

Refilling Capacities＆lubrication

	动臂长度 Boom length
	4600mm
	燃油箱容量Fuel tank
	240L

	斗杆长度Arm length
	2500mm
	冷却系统Cooling system
	20L

	铲斗挖掘Bucket digging force
	97kN
	发动机机油量Engine oil
	12L

	斗杆挖掘力Arm digging force
	70kN
	液压油箱Hydraulic oil tank
	177L

	
	
	系统容量System 
	205L
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           铲斗

Bucket
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    操作重量和接地比压
Operating Weight and Ground Pressure

	型式Type
	Backhoe bucket
	履带板宽度Shoe width
	500mm

	铲斗容量Bucket capacity
	0.6m3 (SAE)
	接地比压Ground pressure
	41.5KPa

	铲斗宽度Bucket width
	1039mm
	操作重量Operating weight
	13320kg

	工作范围Scope of work (mm)
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	A
	最大挖掘高度Max. digging height
	8495mm
	

	B
	最大卸载高度Max. dumping height
	6060mm
	

	C
	最大挖掘深度Max. digging depth
	5490mm
	

	D
	最大垂直挖掘深度

Max. vertical digging depth
	4625mm
	

	E
	挖出2500mm水平面时的最大挖掘深度

Max. Depth cut for 2500mm Level Bottom
	5270mm
	

	F
	最大挖掘距离Max. digging distance
	8300mm
	

	G
	地平面的最大挖掘距离

Max. digging radius at ground level
	8175mm
	

	H
	工作装置最小回转半径

Min. swing radius of work equipment
	2445mm
	

	外形尺寸 Dimensions (mm)                      斗杆长度2500mm

	A
	总长Overall length
	7860mm
	I
	履带轴距 Crawler wheel baHE
	2925mm

	B
	接地长度（运输时）

Ground contact length (Transportation)
	4320mm
	J
	履带长度Track length
	3645mm

	C
	总高（至动臂顶部）

Overall height(to top of boom)
	2800mm
	K
	轨距Track gauge
	2000mm

	D
	总宽Overall width
	2500mm
	L
	履带宽度Track width
	2500mm

	E
	总高（至驾驶室顶部）

Overall height(to top of cab)
	2855mm
	M
	履带板宽度Shoe width
	500mm

	F
	配重离地间隙

Counter weight ground clearance
	915mm
	O
	机罩高度Bonnet height
	2120mm

	G
	最小离地间隙Ground clearance
	425mm
	P
	转台宽度Revolving frame width
	2490mm

	H
	尾部回转半径Tail swing radius
	2380mm
	Q
	回转中心至后端部距离

Distance from swivel center to tail
	2375mm
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